2 0 in a dedicated mixed machine heterogeneous computing hc system an application program may be decomposed into subtasks then each subtask assigned to the machine where it is best suited for execution 
