11 4 the contribution of the former is a tighter schedulability condition which makes more efficient use of network resources than any other existing approaches and that of the latter is a significant improvement in fault tolerance over the basic real time channel which is inherently susceptible to component failures 
