10 5 hence a tsp reads clocks only from a small subset of the tsps in the system which reduces the number of messages by orders of magnitude over a conventional interactive convergence algorithm in which reliable all to all broadcast of clock values is done 
