8 last the complexity of adaptive routers significantly increases their setup delay and flow control cycle times implying that claims of performance advantages in channel utilization and low load latency must be carefully balanced against losses in achievable implementation speed 
